Theory Exam - BSBOHS201A Participate in OHS processes
	Theory Exam - BSBOHS201A Participate in OHS processes
BSBOHS201A 
Participate in OHS processes


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.
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	Date
	29/10/2018





	Number of questions
	Number of questions answered correctly
	Satisfactory?

	24
	
	Yes
	No

	
	
	◻
	◻



	ASSESSOR COMMENTS

	



1. Match the terms and definitions by writing the appropriate letter next to each number in the centre column.

	Answer
	Terms
	Answers
	Definition
	◻

	
	1
	PRA
	1 - F
	A
	Outline the requirements of the work to be undertaken.
	

	
	2
	JSA
	2 - E
	B
	Outline what to do in the event of fires and other accidents
	

	
	3
	Plans and specifications
	3 - A
	C
	Contains important information about hazardous materials or chemicals.
	

	
	4
	Manufacturer specifications
	4 - D
	D
	Outlines how tools and equipment should be used (e.g. lubricant levels, maintenance requirements).
	

	
	5
	SDS
	5 - C
	E
	Identifies hazards and potential hazards that may be encountered while working.
	

	
	6
	Emergency procedures
	6 - B
	F
	A personal assessment of risk
	




2. [bookmark: _Ref424210309][bookmark: _Ref412796746]For each of the hazards identified below, describe the injuries/damage they may cause (i.e. to fellow workers, other people and/or animals) and suggest a suitable control measure.

	Answer
	Hazard
	Injuries or damage
	Control measure
	◻

	
	Hazardous chemical
	Inhaling or contact with the chemical could cause serious medical issues
	PPE, correct storage, labelling, Training.
	

	
	Noise
	Hearing damage, distress, disruption, could cause an incident due it being harder to communicate
	ear muffs (PPE), noise barriers or mufflers on the source, complete the work in specific hours
	

	
	Manual handling
	Sprains, trips and falls
	Training, lift restrictions, tools such as trolleys, etc.
	




3. [bookmark: _Ref415045277]Who should you speak to if you find problems (e.g. hazards, accidents and emergencies)?

	Answer
	A supervisor, manager or health and safety representative
	◻




4. [bookmark: _Ref406591713]What should you do if you discover a fault with plant, tools or equipment?

	Answer
	Stop operation/use, report to supervisor or HS representative, fill out required forms/reporting
	◻





5. [bookmark: _Ref424211517]Which legislation relates to safety in the workplace? Tick your response.

	Answer
	Choice
	Possible Answers
	◻

	
	X
	Occupational Health and Safety Act 2015 
	

	
	x
	Work Health and Safety Act 2011 
	

	
	☐
	Safety Act 1900 
	

	
	☐
	Safety and Health Act 2011 
	




6. [bookmark: _Ref424211632]True or False (Tick your response): Employers are required by legislation to implement safety measures which are reasonably practicable.

	Answer
	x
	True 
	
	◻

	
	☐
	False 
	
	




7. [bookmark: _Ref424211634]True or False (Tick your response): Workers are required by legislation to follow reasonable employer directives (e.g. to undertake first aid and/or fire safety training).

	Answer
	x
	True 
	
	◻

	
	☐
	False 
	
	






8. [bookmark: _Ref424213216]The following symbols appear under the heading ‘Required PPE’ on an SDS. What do the symbols represent?

	Answer
	Symbol
	Meaning
	◻

	
	
[image: ]
	Skin Protection required (long sleeved clothing)
	

	
	
[image: ]
	Hand Protection required
	

	
	
[image: ]
	Eye protection required
	

	
	
[image: ]
	Respiratory Protection required
	




9. [bookmark: _Ref408209094]Describe the meaning and use of the signs displayed below.

	Answer
	Sign
	Meaning
	◻

	
	
	
	

	
	[image: Do Not Enter Saftety Sign]
	Means do not enter the area it is posted outside of. Used to restrict areas to help protect the health and safety of others
	

	
	
	
	






Refer to the Risk Matrix below when responding to Q10. to Q12. 

	Matrix
	A:
Death or permanent disability
	B:
Serious injury
	C:
Lost time injury
	D:
Casualty Treatment
	E:
First Aid

	1: Very Likely
	E
	E
	H
	H
	M

	2: Likely
	E
	H
	H
	M
	M

	3: Possible
	H
	H
	M
	M
	L

	4: Unlikely
	H
	M
	M
	L
	L

	5: Very Unlikely
	M
	M
	L
	L
	L




	E: Extreme
	H: High
	M: Medium
	L: Low





10. [bookmark: _Ref408921283]Which rating is designated for the highest risk and which rating is used for the lowest risk?

	Answer
	Highest  risk  A1 Extreme
Lowest risk E5 Low

	◻





11. [bookmark: _Ref408921265]What is the risk rating for the following circumstances: An event which is possible and would require low-level hospital treatment.

	Answer
	D3 - Medium
	◻





12. [bookmark: _Ref408921287][bookmark: _Ref412797660]What are the factors that would lead to a risk rating of E: Extreme?

	Answer
	A high possibility of the hazard causing serious injury or death
	◻





13. [bookmark: _Ref424212548]When should safety checks be undertaken on machinery and equipment? Tick your response.

	Answer
	Choice
	Possible Answers
	◻

	
	☐
	Before operation
	

	
	☐
	After operation
	

	
	X
	Both before and after operation
	



14. [bookmark: _Ref408921427]Order the elements of the hierarchy of control, from 1 to 6 (i.e. most effective to least effective).
1
2
3
4
5
6


	Answer
	Label (1 – 6)
	Element
	◻

	
	3
	Isolate the hazard
	

	
	6
	Provide and use Personal Protective Equipment (PPE)
	

	
	1
	Eliminate the hazard
	

	
	4
	Control the hazard by engineering means
	

	
	5
	Control the hazard by administrative means
	

	
	2
	Substitute the hazard
	




15. [bookmark: _Ref408921430]Why is elimination the best method of hazard control and PPE considered the least effective?

	Answer
	Eliminating the hazard means that this particular risk is now completely taken away
	◻





16. [bookmark: _Ref408921432]If you were to replace a flammable solvent with a water-based solvent, what category of control measure would that be under the hierarchy of control?

	Answer
	Substitution
	◻




[bookmark: _Ref401921251]


17. [bookmark: _Ref401922320][bookmark: _Ref401900343]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
[image: lifting]F. Hands
E. Knees
D. Shoulders
C. Feet
B. Back
A. Neck

	Answer
	Area of body (Letter)
	How it should be placed
	◻

	
	D
	Level
	

	
	A
	Upright
	

	
	F
	Good grip
	

	
	B
	Natural curve
	

	
	E
	Bent
	

	
	C
	Flat, facing load
	




18. [bookmark: _Ref415049799][bookmark: _Ref421093133]In a medical emergency, what is the first step in the DRSABCD action plan that you need to follow?

	Answer
	Check for danger - checking if there is still a hazard 
	◻





19. [bookmark: _Ref421092991]In the event of a fire emergency, what should you do? 
Fill in the table below to explain the acronym R.A.C.E.

	Answer
	Letter
	Meaning
	◻

	
	R
	Remove people from the area
	

	
	A
	Alert
	

	
	C
	Confine the fire
	

	
	E
	Evacuate
	



20. [bookmark: _Ref414952615]What should you do as part of the clean up process? Tick all that apply.

	Answer
	Choice
	Possible Answers
	◻

	
	☐
	Store all plant, tools and equipment without cleaning
	

	
	X
	Maintain plant, tools and equipment
	

	
	X
	Dispose of materials that cannot be reused or recycled
	

	
	X
	Report faults in logbook and/or site records
	

	
	X
	Clean all plant, tools and equipment before storage
	




21. [bookmark: _Ref408921186]Read the scenario below and complete the Hazard Report Form.

SCENARIO
Today at 10:45am a delivery truck reversed into a car park (located at 54 Standish Street, Salisbury) to deliver gardening materials. There was nobody in the car park to guide the driver and he backed into a number of drums of diesel located to the left of the photograph (below).  One drum was pierced and its contents erupted from the container. 

The marked area on the photo represents the diesel spill, measuring 3m x 4m.












HAZARD REPORT FORM

	GENERAL

	Date
	29/10/18

	Submitted by
	Leilani Kyle

	HAZARD DETAILS

	Location
	54 Standish Street, Salisbury

	Description of issue
	Diesel spill of 3m x 4m caused by a truck backing in to diesel drums.

	Risk class
	☐  Extreme
	☐  High
	x  Medium
	☐  Low

	CONTROL MEASURES

	Corrective action required 
	Contact site personnel, isolate area, spill kit required to clean up, fill in incident report for the site

	Person to action
	Site supervisor, manager and/or HS representative
	When
	X  Immediately
☐  Within 24 hours
☐  Within 7 days




	Answer
	
	◻




22. [bookmark: _Ref412803069]Who would you submit a hazard report form to?

	Answer
	Supervisor, manager or HS representative
	◻





23. [bookmark: _Ref412803089]Who would approve proposed risk controls and organise the required resources for implementation of the risk control?

	Answer
	Supervisor, manager or HS representative
	◻





24. [bookmark: _Ref424215038]Identify one (1) way you can assess if risk controls have been effective.

	Answer
	If hazard has been eliminated in the requested timeframe 
	◻
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