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Handout 1 - Compliance Review

	Participant name
	Abbie Heaslip

	Date
	17/10/24



	Building and construction project
	Southern Queensland Correctional Precinct – Stage 2

	Project overview
	Stage Two involves the construction of a new 1,500-cell, high security facility for male prisoners in Gatton, in order to address growing demand for correctional facilities in Queensland over the next three to five years. 

The Queensland Government declared that this new correctional centre will adopt a ‘health and rehabilitation’ operating model, with the aim of supporting safer communities through enhanced mental health and drug and alcohol rehabilitation services for prisoners, with a particular focus on addressing the ice epidemic and its link to violent and property crime.

	Building classification
	 Class 1 – 10 buildings, max two storeys
 Class 2 – 9 building, Type C only constructions

Specify class: 

	Project site address
	Spring Creek QLD 4343

	State/territory where project is undertaken
	Qld

	Construction plan documents reviewed
	Floor Plan
Structural Drawing (masonry blockwork)
Fire and Electrical Plans
Elevations
Site plan



Building Legislation
List two (2) relevant legislations
	Building legislation
	Plans comply 
	Explanation

	Example: Electrical Safety Act
	 Yes
	 No
	Smoke alarm locations shown in floor plans - photoelectric (AS 3786-2014) hardwired and interconnected.

	Disability (Access to Premises–Building) Standards 2010
	 Yes
	 No
	As shown in the floor plans and other plans and drawings. There is various accessibility provisions included in the Prisons design for prisoners with disabilities.

	Building Fire Safety Regulation 2008
	 Yes
	 No
	As seen in the plans, Smoke alarms are located in each location of the dwellings specified. Stairs, each cell, common areas, etc. All smoke alarms are installed on the ceiling.



Australian Standards
Provide two (2) relevant standards
	Australian Standards
	Plans comply 
	Explanation

	Example: AS/NZS 3786
	 Yes
	 No
	called up in the NCC as the required minimum for smoke alarms to comply with.

	AS 3700
	 Yes
	 No
	sets out the design and construction requirements for masonry structures. referenced in both NCC Volume One and Two providing design and construction requirement for masonry structures.

	AS 1428.1
	 Yes
	 No
	Minimum design and construction requirements for building work in Class 2-9 buildings to enable access for people with disabilities. National Construction Code (NCC) and Disability (Access to Premises – Building) Standards (Premises Standards) refer to this Standard and other Australian Standards as means of compliance with the NCC Deemed-to-Satisfy accessibility provisions.




NCC Requirements
Fire Safety x 1
	Requirements
	Plans comply 
	Explanation

	Volume 1 Section E4V1.
	 Yes
	 No
	Assessment and generation of report in compliance to NCC E4V1.




Health and amenity x 1
	Requirements
	Plans comply 
	Explanation

	Volume 1 Section F2D2
	 Yes
	 No
	Drawings detail caulking to conceal any gaps or spaces which may allow for water to penetrate. Where there is waterproofing and epoxy and what materials used, etc.




Safe movement and access x 1
	Requirements
	Plans comply 
	Explanation

	Volume 1 D4D2

	 Yes
	 No
	Clear in plans and specifications where accessible provisions have been allowed for. Larger beds in accommodation, Reduced height for benches, ramps, disability rooms and areas on ground floor, etc.




Energy efficiency x 1
	Requirements
	Plans comply 
	Explanation

	Volume 1 Section JV3
	 Yes
	 No
	Assessment and generation of report in compliance to NCC J1V3.
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