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ASSESSMENT FOR AHCLSC308

	Student name
	Lopeti Lauaki

	Date of assessment submission
	16/02/2021


	Trainer/Assessor’s name
	

	Date of assessment marking
	Click here to enter a date.
	Outcome for unit
	☐ Competent
☐ Not Yet Competent




TASK INSTRUCTIONS

· As part of the assessment for this unit of competency, you are required to complete a series of activities.
· Some of these activities will require you to provide a response within this document, others will require you to gather evidence to demonstrate your knowledge and skills.
· At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications. 


ACTIVITIES
[bookmark: _Hlk49942093]
	ACTIVITY 1 

	Draw a simple concept plan for a proposed landscape design which includes metal structures/features.




	Response 

	






	Outcome for Activity 1
	☐ Satisfactory 	
☐ Not satisfactory

	Trainer/Assessor comments
	





	ACTIVITY 2 

	Identify/list the detail on the landscape plan shown.

[image: ]





	Response 

	Concrete handball court (5000x5000)
Concrete path (1500wide)
CSBR rubber softball (91sqm)
Astec Mulch Softball (65sqm)
5 x sandstone blocks (500x500x1000)
Concrete edging
Grillex citistyle seat
Grillex Citistyle bin end
Wee saw (wheel chair accessible)
Pentagon swing layout
6 trees (3 large + 3 small)
Concrete edging





	Outcome for Activity 2
	☐ Satisfactory 	
☐ Not satisfactory

	Trainer/Assessor comments
	




	ACTIVITY 3 

	List the materials required to complete the metal structure in the construction plan shown.
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	Response 

	2 x post cap
2 x fence posts
1 x top rail
4 x fence bracket
19 x interlocking pickets
1 x bottom rail
2 x bottom rail cover
24 x 1 5/8 screws





	Outcome for Activity 3
	☐ Satisfactory 	
☐ Not satisfactory

	Trainer/Assessor comments
	





	ACTIVITY 4 

	Have team members take photos and videos of your involvement with metal structures and features. 

Identify each photo / video with a letter label and describe each photo / video in the table below. Submit the photo / video files along with this workbook.




	Advantages

	A
	[image: ] 

Posts and bottom railings have been inserted.  Now we are attaching the panels to create the fence

	B
	[image: ]

Ensuring each part of the panel is attached properly to the post and bottom rail

	C
	[image: ]

Attaching the top rail and ensuring we are using screws to attach each part of the fence.

	D
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	Outcome for Activity 4
	☐ Satisfactory 	
☐ Not satisfactory

	Trainer/Assessor comments
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FosiCap.
(Fla, Crown, o Pyramic)

Fence Post 1

“Top Rall 1

Fence Bracket 4

NOTES:

1. INSTALLATION TO BE COMPLETED PER MANUFACTURER'S
SPECIFICATION.

2. THIS DRAWING IS PROVIDED FOR PLANNING PURPOSES.
REFER TO MANUFACTURER'S INSTALLATIONS FOR
CONSTRUCTION DETALS.

3. REFER TO MANUFACTURER'S WEBSITE FOR PRODUCT
INFORMATION.

4. DRAWING NOT TO SCALE.

TREX SECLUSIONS FENCING
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