 


 
ASSESSMENT FOR 

	Student name
	Kevin Larney

	Date of assessment submission



	Trainer/Assessor’s name
	Tui

	Date of assessment marking

	Outcome for unit
	 Competent
 Not Yet Competent




TASK INSTRUCTIONS

· As part of the assessment for this unit of competency, you are required to complete a series of activities.
· Some of these activities will require you to provide a response within this document, others will require you to gather evidence to demonstrate your knowledge and skills.
· At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications. 
 

ACTIVITIES

	· 

	Identify/list the scope of the work to be carried out from the concept plan shown.








	Response 

	Storage, deck, paved area, pod, screen, pedestrian access, entry, buffer planting, parking auto access, garage, public area and screen. 




	Outcome for Activity 1
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	Identify/list the detail on the landscape plan shown.








	Response 

	Summary and implications, scale, notes, date, north direction and map.




	Outcome for Activity 2
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 



















	· 

	Using the graphics shown, create a simple plan that details a paved path through a garden with grass, trees, shrubs, rocks and steps.








	Response 

	
[image: ]




	Outcome for Activity 3
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	Research the advantages and disadvantages of concrete, clay and stone pavers. 

For each material, provide one (1) example of a project where it would be most appropriate to use the material and one (1) example of a project where it would not be appropriate to use the material. Explain your responses.




	Concrete pavers

	Appropriate

	Versatility, low material and installation cost, many shapes and colours. 
Areas with extreme temperature changes or heavy foot traffic.

	Not appropriate

	It is porous and is susceptible to stains if not resealed regularly.



	Clay pavers 

	Appropriate

	Natural, don't fade in the sun, slip resistant, strong and recyclable. 
Garden pathways, driveways sidewalks, patios and garden walls


	Not appropriate

	High cost, durability issues and maintenance requirements.



	Stone pavers 

	Appropriate

	Provide enhanced aesthetic value, versatile and long lasting durability.
Any area requiring a hardscape that needs to be both beautiful and permeable.

	Not appropriate

	Pavers become uneven over time, not suitable for use around a swimming pool.




	Outcome for Activity 4
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	Obtain photographs of common landscaping materials and finished landscapes (both soft and hard). 

Explain the differences between your emotions/feelings when you see each photograph in black and white and in colour.




	Photograph 1

	
[image: ]

	Black and white: Emotions and feelings

	Simplicity: In black and white, the photograph may evoke a sense of simplicity and minimalism. Without the distraction of colour, the focus shifts to the textures, patterns, and shapes of the pavers. This simplicity can evoke feelings of clarity and calmness. 

	Colour: Emotions and feelings

	Realism: Colour photography provides a more realistic representation of the pavers, allowing the viewer to perceive the materials as they would appear in real life. The colours convey a sense of authenticity and depth, immersing the viewer in the scene. 




	Photograph 2

	[image: ]


	Black and white: Emotions and feelings

	Texture and Contrast: In black and white, the texture of the gravel becomes more pronounced, and the contrast between light and dark areas can be heightened. This emphasis on texture and contrast can evoke feelings of depth and tactility, as the viewer's attention is drawn to the varying shapes and sizes of the gravel particles. 

	Colour: Emotions and feelings

	Naturalism and Realism: Colour photography provides a more realistic representation of the gravel, allowing the viewer to perceive the nuances of colour and texture as they would appear in real life. This sense of naturalism can evoke feelings of connection to nature and an appreciation for the beauty of the outdoors.




	Photograph 3

	[image: ]


	Black and white: Emotions and feelings

	Simplicity and Elegance: The absence of colour in black and white photography can create a sense of simplicity and elegance. Without the distraction of colour, the focus is on the forms and shapes of the plants, fostering a contemplative mood and a sense of sophistication.

	Colour: Emotions and feelings

	Naturalism and Realism: Colour photography provides a more realistic representation of the plants, allowing the viewer to perceive the nuanced colours and textures as they would appear in real life. This sense of naturalism can evoke feelings of connection to nature and an appreciation for the beauty of the outdoors.




	Photograph 4

	[image: Eucalyptus Chips Mulch | Waratah Supplies | Shop Online for Delivery ...]


	Black and white: Emotions and feelings

	Texture and Contrast: In black and white photography, the texture of the mulch becomes more pronounced, and the contrast between light and dark areas can be heightened. This emphasis on texture and contrast can evoke feelings of depth and tactility, as the viewer's attention is drawn to the varying shapes and sizes of the mulch particles.

	Colour: Emotions and feelings

	Naturalism and Realism: In contrast to black and white, a colour photograph of mulch presents the scene with naturalism and realism. The various hues and tones within the mulch, ranging from warm browns to earthy reds and greys, add depth and richness to the image, enhancing its visual appeal and creating a more lifelike representation of the material.




	Outcome for Activity 5
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	



 


	· 

	Research and identify eight (8) different paving patterns, including the common usage, advantages and disadvantages for each pattern.




	Pattern 1 name
	Stack bond

	Common usage

	Used for paving feature sections such as entertaining areas and patios.

	Advantages

	It can look excellent and act as a focal point for the eye.

	Disadvantages

	Not as strong as other paving methods.



	Pattern 2 name
	Running bond

	Common usage

	Used for basic wall construction found in walls and buildings of all kinds.

	Advantages

	Simple, straightforward and strong.

	Disadvantages

	Alignment issues, cracking and shifting and uneven visual flow.




	Pattern 3 name
	Circular Pattern 

	Common usage

	Used for creating focal points in landscaping, including patios, garden pathways, and decorative areas. 

	Advantages

	Adds visual interest and breaks the monotony of straight lines, suitable for enhancing the aesthetic appeal of outdoor spaces.

	Disadvantages

	Requires careful planning and precise cutting, can be challenging to install properly, may not be practical for large areas.




	Pattern 4 name
	Random stone pattern

	Common usage

	Mimics the appearance of natural stone, commonly used for patios, pool decks, and garden pathways.

	Advantages

	Provides a natural and rustic look, hides imperfections well, offers flexibility in design.

	Disadvantages

	Requires careful selection and arrangement of stones, can be time-consuming to install, may be more expensive than other patterns.




	Pattern 5 name
	Herringbone

	Common usage

	Often used for driveways, pathways, and patios, especially in areas with heavy foot traffic.

	Advantages

	Provides better interlocking, increasing stability, visually appealing with its diagonal arrangement, hides imperfections well.

	Disadvantages

	Requires more precise cutting during installation, can be more time-consuming and expensive, not ideal for large areas due to complexity.




	Pattern 6 name
	Hexagonal

	Common usage

	Suitable for pathways, sidewalks, and outdoor areas where a geometric design is desired.

	Advantages

	Offers a visually striking and modern appearance, provides good stability and interlocking, allows for creative design variations.

	Disadvantages

	Requires precise cutting to achieve proper alignment, can be labour-intensive to install, may not suit all architectural styles.




	Pattern 7 name
	Basketweave

	Common usage

	Popular for patios, walkways, and small to medium-sized outdoor spaces.

	Advantages

	Offers a unique and visually interesting design, provides good traction due to its interlocking nature.

	Disadvantages

	May not be as strong as some other patterns, requires regular maintenance to prevent weeds from growing in the open areas.




	Pattern 8 name
	Irregular pattern

	Common usage

	Offers a natural and organic look, often used for pathways, garden walkways, and rustic outdoor spaces.

	Advantages

	Mimics the randomness of natural stone formations, hides imperfections well, allows for creative and unique designs.

	Disadvantages

	Requires careful planning to achieve a balanced appearance, may result in uneven surfaces if not installed properly, can be more challenging to maintain over time.




	Outcome for Activity 6
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	



 

	· 

	Select a paver type (with known specifications) and calculate the material costs for a straight path that measures 6m long by 900mm wide.




	Response 

	Let's choose a common paver type: concrete pavers. Typically, concrete pavers come in standard sizes such as 200mm x 100mm x 50mm.

Given the dimensions of the path (6m long by 900mm wide), we need to calculate the number of pavers required.

Convert dimensions to meters:

Length: 6 meters
Width: 0.9 meters
Determine paver coverage area:

Each paver covers an area of (0.2m x 0.1m) = 0.02 square meters.
Calculate the total area of the path:

Total area = Length x Width = (6m x 0.9m) = 5.4 square meters.
Determine the number of pavers needed:

Number of pavers = Total area / Paver coverage area = 5.4 sqm / 0.02 sqm = 270 pavers.
Now, let's calculate the material costs:

Cost of Concrete Pavers:

Prices for concrete pavers can vary depending on quality, brand, and location. Let's assume a cost of $3 per paver.
Total Cost of Pavers = Number of Pavers × Cost per Paver
= 270 pavers × $3/paver
= $810

So, the material cost for a straight path measuring 6m long by 900mm wide using concrete pavers would be approximately $810.




	Outcome for Activity 7
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	Research the advantages and disadvantages of installing edging before and after laying pavers.




	Installing edging before laying pavers

	Advantages

	Guidance and Stability: Installing edging beforehand provides a clear boundary for laying pavers, ensuring they stay in place and preventing shifting over time.
Ease of Installation: It can be easier to install the edging before laying the pavers, as there's more space to work with and adjust the placement of the edging.

	Disadvantages

	Limited Flexibility: Installing edging before laying pavers may limit flexibility in the design or layout adjustments, as the edging determines the boundary of the paved area.
Increased Planning Required: Precise planning is necessary to ensure the edging is properly aligned and leveled before laying the pavers, which can add time to the project's preparation phase.



	Installing edging after laying pavers 

	Advantages

	Flexibility in Design: Installing edging after laying pavers allows for more flexibility in adjusting the layout or design, as the pavers can be arranged first and the edging can be customized to fit the specific shape and size of the paved area.
Easier Alignment: It can be easier to align and adjust the edging to fit the contours of the paved area once the pavers are already in place.

	Disadvantages

	Potential for Shifting: Without edging in place during paver installation, there's a risk of pavers shifting or spreading out of place over time, especially in areas with heavy foot traffic or vehicle loads.
Weed Growth: Delaying the installation of edging may allow for weed growth between the pavers before edging is installed, requiring additional maintenance to address weed issues.




	Outcome for Activity 8
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	



 

	· 

	List environmentally safe products for cleaning.




	Response 

	Vinegar: Vinegar is a natural and versatile cleaner that can effectively dissolve grease, soap scum, and mineral deposits. It's safe for most surfaces except for marble and other sensitive stones.
Baking Soda: Baking soda is a mild abrasive that can be used to scrub surfaces, deodorize carpets, and neutralize odours in refrigerators and other areas. It's non-toxic and safe for the environment.
Castile Soap: Made from vegetable oils, castile soap is gentle on the skin and safe for the environment. It can be used for general cleaning, dishwashing, laundry, and even personal hygiene.
Hydrogen Peroxide: Hydrogen peroxide is a natural disinfectant and bleach alternative that can be used to kill germs, whiten laundry, and remove stains. It breaks down into water and oxygen, making it safe for the environment.
Lemon Juice: Lemon juice is acidic and has natural antibacterial properties, making it effective for cutting through grease and disinfecting surfaces. It also leaves a fresh citrus scent.





	Outcome for Activity 9
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	Have team members take photos and videos of your involvement with paving projects. 

Identify each photo / video with a letter label and describe each photo / video in the table below. Submit the photo / video files along with this workbook.




	Advantages

	A
	

	B
	

	C
	

	D
	

	E
	

	F
	

	G
	

	H
	

	I
	

	J
	

	K
	

	L
	

	M
	

	N
	

	O
	

	P
	

	Q
	

	R
	

	S
	

	T
	

	U
	

	V
	

	W
	

	X
	

	Y
	

	Z
	




	Outcome for Activity 10
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
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